**Description:**

Type: BROEN BALLOMAX

Art. No.: 94.100

Pressure: PN 40

Dimension: DN 010 to DN 050

**Configuration:**

Fully welded ball valve with full bore and female/female connection. Especially designed for use in central heating, heating, cooling and industrial plants. Stem and stop made in stainless steel with double sealings in stuffing box with exchangeable o-rings. The valves are approved according to the directive for pressurized equipment PED 2014/68/EU, Module H. and manufactured according to ISO9001:2008 and ISO14001.

**Technical data:**

Connection: Female/Female

Temperature: Continuously 140 °C

Media: Treated water to avoid corrosion/lime formation

House: Steel P235GH (St. 37)

O-rings: EPDM and VITON

Ball: Stainless Steel AISI 304L

Seat packing: Reinforced PTFE 20% C

Operation: Handle

Surface: Environmentally friendly corrosion resistant paint

**Labeling:**

Maker, Dimension, Pressure step, Temperature range, Production month and year.

CE marking

**Accessories:**

T-handle in Yellow, Red and/or Blue