**Description:**

Type: BROEN BALLOMAX

Art. No.: 69.300.V…

Pressure: PN 40

Dimension: DN 015 to DN 032

**Configuration:**

Main stop valves mounted on a heavy steel bracket with possible adjustable mounting on wall and variable adjustment of the valves individual location.

Fully welded ball valve with reduced bore and female/female connection. Especially designed for use in central heating, anglepositioned for TWIN-pipes. Stem and stop made in stainless steel with double sealings in stuffing box with exchangeable o-rings.

The valves are approved according to the directive for pressurized equipment PED 2014/68/EU, Module H. and manufactured according to ISO9001:2008 and ISO14001.

**Technical data:**

Connection: Female / Female

Temperature: Continuous 140 °C

Media: Treated water to avoid corrosion/lime formation

House: Steel P235GH (St. 37)

O-rings: EPDM and VITON

Ball: Stainless Steel AISI 304L

Seat packing: Reinforced PTFE 20%C

Operation: T-handle Red/Blue, reversible

Surface: Environmentally corrosion resistant paint

**Labeling:**

Maker, Dimension, Pressure step, Temperature range, Production month and year.

CE marked

**Accessories:**

Yellow T-handle

DN020 & DN025 insulations shells

Extra bracket for extension

Locking bracket